
<https://www.youtube.com/watch?v=4R6qdBgm_JQ>



CODE

int relayPin=8;

void setup() {

pinMode(relayPin,OUTPUT);

digitalWrite(relayPin,LOW);// put your setup code here, to run once:

}

void loop() {

digitalWrite(relayPin,HIGH);// put your main code here, to run repeatedly:

delay(2000);

digitalWrite(relayPin, LOW);

delay(2000);

}