<https://www.youtube.com/watch?v=4R6qdBgm_JQ>



CODE

int relayPin=8;

void setup() {

 pinMode(relayPin,OUTPUT);

 digitalWrite(relayPin,LOW);// put your setup code here, to run once:

}

void loop() {

 digitalWrite(relayPin,HIGH);// put your main code here, to run repeatedly:

 delay(2000);

 digitalWrite(relayPin, LOW);

 delay(2000);

}